Grading node:

PosS: Start position  
PosT: Target position  
Sm: Max speed of any transportation (130km/h).

Grading edge:  
S: Max speed of current transport system.  
C: Must change vehicle (0 or 1)  
x: vehicle change constant.  
PosA: A positon  
PosB: B positon